APPENDIX No. 1. TECHNICAL SPECIFICATION
Functional and technical parameters of the granite aggregate processing plant:
	Item No.
	Functional and technical parameters
	Parameter values

	1
	2
	3

	1. 
	Processing plant capacity and products
	The granite aggregate processing plant operates efficiently at a capacity of 310 t/h when producing 0/22 mm material and at 230 t/h when producing 0/16 material. The plant is designed to produce the following fractions: 0/2, 2/5, 5/8, 8/11, 11/16 and 16/22.

	2. 
	FLSmidth Raptor 450 cone crusher
	· capacity: 190–650 t/h;
· power supply: 400/690 V, 50 Hz;
· maximum size of material to be crushed: 270 mm;
· minimum size of material to be crushed: 5 mm;
· electric motor power: 320 kW;
· electric motor speed: 1,400 rpm;
· drive speed: 690 rpm;
· gap between the cones: 10–50 mm;
· hydraulic oil tank capacity: 200 L;
· lubrication tank capacity: 600 L;
· automatic lubrication and hydraulic system;
· protection against uncrushable material;
· crusher control system;
· crusher weight: 33,000 kg;
· crusher height: 3,000 mm

	3. 
	25 m³ hopper with 100 × 300 feeder
	· hopper capacity: 25 m³;
· vibrating feeder nominal size: 1,000 × 3,000 mm;
· vibrating feeder power: 2 × 2.7 kW;
· supporting metal structure, galvanised

	4. 
	Three-deck vibrating screen 240 × 600/3
	· motor power: 2 × 22 kW
· vibrating screen nominal size: 2,400 × 6,000 mm;
· metal screen mesh;
· dust cover, easily removable;
· electric brake;
· galvanised supporting metal structure with maintenance platform;
· armoured metal chutes;

	5. 3.
	Two-deck vibrating screen 240 × 600/2
	· motor power: 30 kW;
· vibrating screen nominal size: 2,400 × 6,000 mm;
· metal screen mesh;
· dust cover, easily removable;
· electric brake;
· galvanised supporting metal structure with maintenance platform;
· armoured metal chutes;

	6. 
	Two-deck vibrating screen 240 × 700/2
	· motor power: 37 kW;
· vibrating screen nominal size: 2,400 × 7,000 mm;
· metal screen mesh;
· dust cover, easily removable;
· electric brake;
· galvanised supporting metal structure with maintenance platform;
· armoured metal chutes;

	7. 
	Stationary conveyor T-1
	· Covered conveyor with galvanised structure;
· Maintenance walkway on one side;
· Length: 10 m;
· Belt width: 1 000 mm;
· Angle: 7°;
· Capacity: 320 t/h;
· Power: 5,5 kW;
· Belt speed: 1,27 m/s

	8. 
	Stationary conveyor T-2
	· Covered conveyor with galvanised structure;
· Maintenance walkways on both sides;
· Length: 31 m;
· Belt width: 1 000 mm;
· Angle: 14°;
· Capacity: 345 t/h;
· Power: 2 × 11,0 kW;
· Belt speed: 1,18 m/s

	9. 
	Stationary conveyor T-3
	· Covered conveyor with galvanised structure;
· Maintenance walkways on both sides;
· Length: 55 m;
· Belt width: 650 mm;
· Angle: 18/3°;
· Capacity: 96 t/h;
· Power: 2 × 7,5 kW;
· Belt speed: 1,14 m/s

	10. 
	Stationary conveyor T-4
	· Covered conveyor with galvanised structure;
· Maintenance walkway on one side;
· Length: 8 m;
· Belt width: 650 mm;
· Angle: 5°;
· Capacity: 96 t/h;
· Power: 2,2 kW;
· Belt speed: 1,10 m/s

	11. 
	Slewing conveyor T-5
	· Covered conveyor with galvanised structure;
· Maintenance walkway on one side;
· Length: 25 m;
· Belt width: 800 mm;
· Angle: 18°;
· Capacity: 147 t/h;
· Power: 2 × 5,5 kW;
· Slewing mechanism: 0,75 kW;
· Belt speed: 1,34 m/s

	12. 
	Stationary conveyor T-6
	· Covered conveyor with galvanised structure;
· Length: 7 m;
· Belt width: 650 mm;
· Angle: 15°;
· Capacity: 69 t/h;
· Power: 3 kW;
· Belt speed: 1,15 m/s

	13. 
	Slewing conveyor (T-7, T-15), 2 units
	· Covered conveyor with galvanised structure;
· Maintenance walkway on one side;
· Length: 25 m;
· Belt width: 650 mm;
· Angle: 18°;
· Capacity: 63–69 t/h;
· Power: 7,5 kW;
· Slewing mechanism: 0,75 kW;
· Belt speed: 1,34 m/s

	14. 
	Stationary conveyor T-8
	· Covered conveyor with galvanised structure;
· Length: 10 m;
· Belt width: 1 000 mm;
· Angle: 15°;
· Capacity: 230 t/h;
· Power: 7,5 kW;
· Belt speed: 1,14 m/s

	15. 
	Stationary conveyor T-9
	· Covered conveyor with galvanised structure;
· Maintenance walkways on both sides;
· Length: 57 m;
· Belt width: 1 000 mm;
· Angle: 18/0°;
· Capacity: 230 t/h;
· Power: 2 × 15 kW;
· Belt speed: 1,18 m/s

	16. 
	Stationary conveyor T-10
	· Covered conveyor with galvanised structure;
· Maintenance walkways on both sides;
· Length: 40 m;
· Belt width: 800 mm;
· Angle: 18/0°;
· Capacity: 142 t/h;
· Power: 2 × 9,2 kW;
· Belt speed: 1,16 m/s

	17. 
	Stationary conveyor T-11
	· Covered conveyor with galvanised structure;
· Length: 6 m;
· Belt width: 650 mm;
· Angle: 13°;
· Capacity: 50 t/h;
· Power: 3 kW;
· Belt speed: 1,15 m/s

	18. 
	Slewing conveyor (T-12, T-16, T-19), 3 units
	· Covered conveyor with galvanised structure;
· Maintenance walkway on one side;
· Length: 25 m;
· Belt width: 650 mm;
· Angle: 18°;
· Capacity: 38–50 t/h;
· Power: 7,5 kW;
· Slewing mechanism: 0,75 kW;
· Belt speed: 1,34 m/s

	19. 
	Stationary conveyor (T-13, T-17), 2 units
	· Covered conveyor with galvanised structure;
· Length: 10 m;
· Belt width: 650 mm;
· Angle: 15°;
· Capacity: 38 t/h;
· Power: 3 kW;
· Belt speed: 1,15 m/s

	20. 
	Stationary conveyor T-14
	· Covered conveyor with galvanised structure;
· Length: 27 m;
· Belt width: 650 mm;
· Angle: 7°;
· Capacity: 38 t/h;
· Power: 5,5 kW;
· Belt speed: 1,08 m/s

	21. 
	Stationary conveyor T-18
	· Covered conveyor with galvanised structure;
· Length: 20 m;
· Belt width: 650 mm;
· Angle: 9°;
· Capacity: 38 t/h;
· Power: 4 kW;
· Belt speed: 1,07 m/s

	22. 
	Dust-suppression water spraying system
	· designed for and installed on the granite aggregate processing plant;
· installed on the movable conveyors at the discharge points into the stockpiles (6 points);
· the dust-suppression water spraying system is integrated with the control system of the entire processing plant.
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          1   PRIEDAS Nr. 1 .  TECHNINĖ SPECIFIKACIJA   Granit o   skaldos technologinės linijos funkciniai ir techniniai rodikliai :  

Eil.  Nr.  Funkciniai ir techniniai rodikliai  Rodiklių reikšmės  

1  2  3  

1.    Technologinės linijos našumas, pro- dukcija  Granito skaldos technologinė linija efektyviai veiki a   310 t/h našumu ga- minant 0/22 mm ir 230 t/h našumu gaminant 0/16 produkciją. Linija  pri- taikyta ir skirta gaminti   fr. 0/2, 2/5, 5/8, 8/11, 11/16, 16/22.  

2.    Kūginis trupintuvas  FLSmidth Raptor  450     našumas 190  -   650 t/h;      el. maitinimas 400/690 V 50 Hz;      trupinamos medžiagos   maksimalus   dydis 270 mm;      trupinamos medžiaga   minimalus   dydis 5 mm;      el. variklio galia   320 kW;      el. variklio greitis 1400 aps./min;      pavaros greitis 690 aps./min;      tarpas tarp kūgių  nuo   10 mm i ki   50 mm;      hidraulinio tepalo talpos dydis 200 L;      tepimo bako talpos dydis   600 L;      automatinė tepimo ir hidraulinė sistema;      apsauga nuo netrupinamos medžiagos;      trupintuvo valdymo sistema;      trupintuvo svoris 33000 kg;      trupintuvo aukštis   3000 mm  

3.    Bunkeris 25 m 3   su maitintuvu 100x300     bunkerio talpa 25 m 3 ;      vibruojančio  maitintuvo nominalus dydis 1000x3000 mm;      vibruojančio maitintuvo galingumas 2x2,7 kW;      laikančioji   metalinė konstrukcija (cinkuota)  

4.    Trijų lygių vibrosijotuvas 240x600/3     variklio galingumas 2x22 kW      vibrosijotuvo nominalus dydis 2400x6000 mm;      sietas - metalinis;      dangtis nuo dulkėjimo (lengvai nuimamas);      el. stabdis;      laikančioji metalinė konstrukcija (cinkuota) su aptarnavimo aikš- tele;      šarvuoti metaliniai latakai;  

5.   3 .  Dviejų lygių vibrosijotuvas 2 4 0x600/2     variklio galingumas  30   kW;      vibrosijotuvo nominalus dydis 2 4 00x6000 mm;      sietas - metalinis;      dangtis nuo dulkėjimo (lengvai nuimamas);      el. stabdis;      laikančioji metalinė konstrukcija (cinkuota) su aptarnavimo aikš- tele;      šarvuoti metaliniai latakai;  

6.    Dviejų lygių vibrosijotuvas 240x 7 00/2     variklio galingumas  37   kW;      vibrosijotuvo nominalus dydis 2400x 7 000 mm;      sietas - metalinis;      dangtis nuo dulkėjimo (lengvai nuimamas);      el. stabdis;      laikančioji metalinė konstrukcija(cinkuota) su aptarnavimo aikš- tele;      šarvuoti metaliniai latakai;  

7.    Stacionarus konvejeris T - 1     Dengtos konstrukcijos konvejeris, su  cinkuota konstrukcija;       Aptarnavimo takelis iš vienos pusės;      Ilgis 10 m;      Juostos plotis 1000 mm;      Kampas   7 ⁰;  

