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Caterpillar D6T XL Crawler Tractor
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Dimensions

Dimensions

. Width Over Tracks

. Height To Top Of Cab

. Length Of Track On Ground
. Ground Clearance

. Length W/0 Blade

Undercarriage
. Standard Shoe Size
Ground Pressure
Track Pitch
Ground Contact Area
Number Of Track Rollers Per Side

Number Of Shoes Per Side

8ftin

10.5ftin

9.42ftin

1.25ftin

12.67 ftin

22in

8.9 psi

8in

4972in2

4
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Specifications

Engine

Number Of Cylinders
Engine Make

Engine Model

Gross Power

Net Power

Power Measured @

Displacement

Operational

Operating Weight

Fuel Capacity

Cooling System Fluid Capacity
Engine Oil Capacity

Hydraulic Fluid Capacity
Powertrain Fluid Capacity
Final Drives Fluid Capacity
Operating Voltage

Alternator Supplied Amperage

2236

C9 ACERT

228 hp

199.9hp

1850 rpm

537cuin

447951b

112 gal

18.5gal

7.4 gal

13.6 gal

38.5gal

3.6gal

24V

95amps
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Transmission
Transmission Type
Number Of Forward Gears
Number Of Reverse Gears
Max Speed - Forward
Max Speed - Reverse

Hydraulic System

Relief Valve Pressure

Pump Flow Capacity

Standard Blade

Width

Height

Capacity

Cutting Depth

Powershift

7.2 mph

9.1 mph

2799 psi

49.9 gal/min

13.7 ftin

45in

5.2yd3

21in




