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Caterpillar D9T Crawler Tractor
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Dimensions

Dimensions

@ Length W/ Blade 21.76ftin
. Width Over Tracks 9.4ftin
@© Height To Top Of Cab 12.5ftin
. Length Of Track On Ground 11.4ftin
. Ground Clearance 1.96 ftin
@ Length W/0 Blade 16.11 ftin

Undercarriage

. Track Gauge 7.39ftin

. Standard Shoe Size 24in
Number Of Shoes Per Side 43
Ground Pressure 16.08 psi
Ground Contact Area 6569 in2
Number Of Track Rollers Per Side 8

Track Pitch 9.44in
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Specifications

Engine

Engine Make
Engine Model
Gross Power

Net Power

Power Measured @

Displacement

Operational

Operating Weight

Fuel Capacity

Cooling System Fluid Capacity
Engine Oil Capacity

Hydraulic Fluid Capacity
Powertrain Fluid Capacity
Final Drives Fluid Capacity
Operating Voltage

Alternator Supplied Amperage

2236

C18 ACERT

464hp

410hp

1800 rpm

1106 cuin

105600 Ib

235gal

27.5gal

10 gal

23.5gal

43.4gal

3.9gal

24V

95amps
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Transmission
Transmission Type
Number Of Forward Gears
Number Of Reverse Gears
Max Speed - Forward

Max Speed - Reverse

Hydraulic System
Pump Type
Relief Valve Pressure

Pump Flow Capacity

Standard Blade

Width

Height

Capacity

Cutting Depth

Power Shift

7.3 mph

8.9 mph

Piston

5875 psi

101 gal/min

14.3ftin

6.5in

17.7yd3

23.9in




