[image: ]IDECO SBS 

Manufactured in 1966 / Recertified in 1989/2001
Serial number 163
Manufactured in the USA

MAST
Type					KM 90/95 – 180 GH
Clear Height				95 ft (29 m)
Max. Hook Load Capacity			250,000 lbs (112 t) 

SUBSTRUCTURE
Type					IDECO SBS	
[image: ]Setback Capacity			220,000 lbs (100 t)
Rotary Capacity				250,000 lbs (112 t)
Height underneath Rotary Beams		9 ft (2.9 m)

DRAWWORKS
Type					IDECO H35ED
Max. Line Pull, 2nd Layer			30,000 lbs (13,5 t)
Drilling Line				1 in
Rated Input Power			350 HP
Auxiliary Brake				Hydromat
Drive					Detroit Diesel 12V71-N

RIG POWER SYSTEM
Drive					Diesel
Type of Engines				1 x Detroit Diesel 12V71-N (drawwarks)
Nominal Rated Power	 		396 HP

MUD PUMPS
Type (Triplex Pumps)			EMSCO  F500
Number				2

ROTARY TABLE
Type					SK 175

[bookmark: _Hlk115780156]BLOCK
Type					Block Mc Kissick 150
Capacity				150 t

MUD TANK SYSTEM
Number			2	
Capacity				80 m³
					LP Mixing System,
					Mud Agitators,
					Degasser

SOLIDS CONTROL EQUIPMENT
Type					2 x SWACO Mongoose
					Shale Shaker
Type					1 x 10" Desander
Type					10 x 4" Desilter
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